Current configuration:
!
version 12.0
service timestamps debug uptime
service timestamps log uptime
no service password-encryption
!
hostname Router-B
!
enable secret 5 $1$Z2Bx$YWjQ4FouiajB/fEw8srJb.
!
!
ip subnet-zero
!
ip audit notify log
ip audit po max-events 100
!
process-max-time 200
!
interface FastEthernet0/0
 ip address 10.0.0.1 255.0.0.0
 no ip directed-broadcast
!
interface Serial0/0
 ip address 3.0.0.1 255.255.255.0
 no ip directed-broadcast
 no ip mroute-cache
 no fair-queue
 clockrate 56000
!
interface Serial0/1
 ip address 2.0.0.1 255.255.255.0
 no ip directed-broadcast
 clockrate 56000
!
router eigrp 300
 network 2.0.0.0
 network 10.0.0.0
!
router bgp 300
 no synchronization
 network 10.0.0.0
 neighbor 2.0.0.2 remote-as 300
 neighbor 2.0.0.2 next-hop-self
 neighbor 3.0.0.2 remote-as 200
!
ip classless
no ip http server
!
!
line con 0
 transport input none
line aux 0
line vty 0 4
 password cisco
 login
!
no scheduler allocate
end
