Output=RTA%23show+running%2Dconfig%0Ahostname+RTA%0A%0Aip+subnet%2Dzero%0A%0Ainterface+Loopback0%0A+ip+address+203%2E250%2E13%2E41+255%2E255%2E255%2E0%0A%0Ainterface+Ethernet0%0A+ip+address+203%2E250%2E14%2E1+255%2E255%2E255%2E0%0A%0Ainterface+Serial0%0A+ip+address+128%2E213%2E63%2E1+255%2E255%2E255%2E252%0A%0Arouter+ospf+10%0A+redistribute+bgp+100+metric+2000+subnets%0A+passive%2Dinterface+Serial0%0A+network+203%2E250%2E0%2E0+0%2E0%2E255%2E255+area+0%0A+network+128%2E213%2E0%2E0+0%2E0%2E255%2E255+area+0%0A+default%2Dinformation+originate+metric+2000%0A%0Arouter+bgp+100%0A+no+synchronization%0Anetwork+203%2E250%2E13%2E0%0A+network+203%2E250%2E14%2E0%0A+neighbor+128%2E213%2E63%2E2+remote%2Das+200%0A+neighbor+128%2E213%2E63%2E2+route%2Dmap+setlocalpref+in%0A+neighbor+203%2E250%2E15%2E2+remote%2Das+100%0A+neighbor+203%2E250%2E15%2E2+update%2Dsource+Loopback0%0A%0Aip+classless%0Aip+default%2Dnetwork+200%2E200%2E0%2E0%0A%0Aroute%2Dmap+setlocalpref+permit+10%0A+set+local%2Dpreference+200%0A%0ARTA%23%0A