
vlanDBC.addSC("abort", "Exit mode without applying the changes");
vlanDBC.addSC("apply", "Apply current changes and bump revision number");
vlanDBC.addSC("exit", "Apply changes, bump revision number, and exit mode");
vlanDBC.addSC("no", "Negate a command or set its defaults");
	vlanDBC.no.addSC("abort", "Exit mode without applying the changes");
	vlanDBC.no.addSC("apply", "Apply current changes and bump revision number");
	vlanDBC.no.addSC("exit", "Apply changes, bump revision number, and exit mode");
	vlanDBC.no.addSC("reset", "Abandon current changes and reread current database");
	vlanDBC.no.addSC("show", "Show database information");
		vlanDBC.no.show.addSC("changes", "Show the changes to the database since modification began (or since 'reset')");
			vlanDBC.no.show.changes.addSC("<1-1005>", "ID number of the VLAN shown");
		vlanDBC.no.show.addSC("current", "Show the database installed when modification began (or since 'reset')");
			vlanDBC.no.show.current.addSC("<1-1005>", "ID number of the VLAN shown");
		vlanDBC.no.show.addSC("proposed", "Show the database as it would be modified if applied");
			vlanDBC.no.show.proposed.addSC("<1-1005>", "ID number of the VLAN shown");
	vlanDBC.no.addSC("vlan", "Add, delete, or modify values associated with a single VLAN");
		vlanDBC.no.vlan.addSC("<1-1005>", "ISL VLAN index");
			vlanDBC.no.vlan["<1-1005>"].addSC("are", "Maximum number of All Route Explorer hops for this VLAN (or zero if none specified)");
			vlanDBC.no.vlan["<1-1005>"].addSC("backupcrf", "Backup CRF mode of the VLAN");
			vlanDBC.no.vlan["<1-1005>"].addSC("bridge", "Bridging characteristics of the VLAN");
			vlanDBC.no.vlan["<1-1005>"].addSC("media", "Media type of the VLAN");
			vlanDBC.no.vlan["<1-1005>"].addSC("mtu", "VLAN Maximum Transmission Unit");
			vlanDBC.no.vlan["<1-1005>"].addSC("name", "Ascii name of the VLAN");
			vlanDBC.no.vlan["<1-1005>"].addSC("parent", "ID number of the Parent VLAN of FDDI or Token Ring type VLANs");
			vlanDBC.no.vlan["<1-1005>"].addSC("ring", "Ring number of FDDI or Token Ring type VLANs");
			vlanDBC.no.vlan["<1-1005>"].addSC("said", "IEEE 802.10 SAID");
			vlanDBC.no.vlan["<1-1005>"].addSC("state", "Operational state of the VLAN");
			vlanDBC.no.vlan["<1-1005>"].addSC("ste", "Maximum number of Spanning Tree Explorer hops for this VLAN (or zero if none specified)");
			vlanDBC.no.vlan["<1-1005>"].addSC("stp", "Spanning tree characteristics of the VLAN");
			vlanDBC.no.vlan["<1-1005>"].addSC("tb-vlan1", "ID number of the first translational VLAN for this VLAN (or zero if none)");
			vlanDBC.no.vlan["<1-1005>"].addSC("tb-vlan2", "ID number of the second translational VLAN for this VLAN (or zero if none)");
	vlanDBC.no.addSC("vtp", "Perform VTP administrative functions.");
		vlanDBC.no.vtp.addSC("client", "Set the device to client mode.");
		vlanDBC.no.vtp.addSC("password", "Set the password for the VTP administrative domain.");
		vlanDBC.no.vtp.addSC("pruning", "Set the administrative domain to permit pruning.");
			vlanDBC.no.vtp.pruning.addSC("v2-mode", "Set the administrative domain to V2 mode.");
		vlanDBC.no.vtp.addSC("transparent", "Set the device to transparent mode.");
		vlanDBC.no.vtp.addSC("v2-mode", "Set the administrative domain to V2 mode.");
vlanDBC.addSC("reset", "Abandon current changes and reread current database");
vlanDBC.addSC("show", "Show database information");
	vlanDBC.show.addSC("changes", "Show the changes to the database since modification began (or since 'reset')");
		vlanDBC.show.changes.addSC("<1-1005>", "ID number of the VLAN shown");
	vlanDBC.show.addSC("current", "Show the database installed when modification began (or since 'reset')");
		vlanDBC.show.current.addSC("<1-1005>", "ID number of the VLAN shown");
	vlanDBC.show.addSC("proposed", "Show the database as it would be modified if applied");
		vlanDBC.show.proposed.addSC("<1-1005>", "ID number of the VLAN shown");
vlanDBC.addSC("vlan", "Add, delete, or modify values associated with a single VLAN");
	vlanDBC.vlan.addSC("<1-1005>", "ISL VLAN index");
		vlanDBC.vlan["<1-1005>"].addSC("are", "Maximum number of All Route Explorer hops for this VLAN");
		vlanDBC.vlan["<1-1005>"].addSC("backupcrf", "Backup CRF mode of the VLAN");
		vlanDBC.vlan["<1-1005>"].addSC("bridge", "Bridging characteristics of the VLAN");
		vlanDBC.vlan["<1-1005>"].addSC("media", "Media type of the VLAN");
		vlanDBC.vlan["<1-1005>"].addSC("mtu", "VLAN Maximum Transmission Unit");
		vlanDBC.vlan["<1-1005>"].addSC("name", "Ascii name of the VLAN");
			vlanDBC.vlan["<1-1005>"].name.addSC("WORD", "The ascii name for the VLAN");
		vlanDBC.vlan["<1-1005>"].addSC("parent", "ID number of the Parent VLAN of FDDI or Token Ring type VLANs");
		vlanDBC.vlan["<1-1005>"].addSC("ring", "Ring number of FDDI or Token Ring type VLANs");
		vlanDBC.vlan["<1-1005>"].addSC("said", "IEEE 802.10 SAID");
		vlanDBC.vlan["<1-1005>"].addSC("state", "Operational state of the VLAN");
		vlanDBC.vlan["<1-1005>"].addSC("ste", "Maximum number of Spanning Tree Explorer hops for this VLAN");
		vlanDBC.vlan["<1-1005>"].addSC("stp", "Spanning tree characteristics of the VLAN");
		vlanDBC.vlan["<1-1005>"].addSC("tb-vlan1", "ID number of the first translational VLAN for this VLAN (or zero if none)");
		vlanDBC.vlan["<1-1005>"].addSC("tb-vlan2", "ID number of the second translational VLAN for this VLAN (or zero if none)");
vlanDBC.addSC("vtp", "Perform VTP administrative functions.");
	vlanDBC.vtp.addSC("client", "Set the device to client mode.");
	vlanDBC.vtp.addSC("domain", "Set the name of the VTP administrative domain.");
		vlanDBC.vtp.domain.addSC("WORD", "The ascii name for the VTP administrative domain.");
	vlanDBC.vtp.addSC("password", "Set the password for the VTP administrative domain.");
		vlanDBC.vtp.password.addSC("WORD", "The ascii password for the VTP administrative");
		vlanDBC.vtp.password.addSC("domain.", "");
	vlanDBC.vtp.addSC("pruning", "Set the administrative domain to permit pruning.");
		vlanDBC.vtp.pruning.addSC("v2-mode", "Set the administrative domain to V2 mode.");
	vlanDBC.vtp.addSC("server", "Set the device to server mode.");
	vlanDBC.vtp.addSC("transparent", "Set the device to transparent mode.");
	vlanDBC.vtp.addSC("v2-mode", "Set the administrative domain to V2 mode.");
