Current configuration:
!
version 12.0
service timestamps debug uptime
service timestamps log uptime
no service password-encryption
!
hostname Router-C
!
enable secret 5 $1$F09j$v93BrmgTG4X/CM3YKcl050
!
!
ip subnet-zero
!
ip audit notify log
ip audit po max-events 100
!
process-max-time 200
!
interface FastEthernet0/0
 ip address 11.0.0.1 255.0.0.0
 no ip directed-broadcast
!
interface Serial0/0
 ip address 3.0.0.2 255.255.255.0
 no ip directed-broadcast
 no ip mroute-cache
 no fair-queue
!
interface Serial0/1
 no ip address
 no ip directed-broadcast
 shutdown
!
router bgp 200
 network 11.0.0.0
 neighbor 3.0.0.1 remote-as 300
!
ip classless
no ip http server
!
!
line con 0
 exec-timeout 0 0
 transport input none
line aux 0
line vty 0 4
 password cisco
 login
!
no scheduler allocate
end
