Content

| 7.6 |  | Network Design Issues for Voice |
| 7.6.7 |  | Implementing IP telephony with auxiliary VLANs |

Auxiliary VLANs and Data VLANs
The new voice VLAN is called an auxiliary VLAN in the Catalyst software command-line interface (CLI). In the traditional switched world, data devices reside in a data VLAN. The new auxiliary VLAN is used to represent other types of devices collectively. Today those devices are IP phones (hence the notion of a voice VLAN), but, in the future, other types of non-data devices will also be part of the auxiliary VLAN. Just as data devices come up and reside in the native VLAN (default VLAN), IP phones come up and reside in the auxiliary VLAN, if one has been configured on the switch.

When the IP phone powers up, it communicates with the switch using CDP. The switch then provides the phone with its configured VLAN ID (voice subnet), also known as the voice VLAN ID or VVID. Meanwhile, data devices continue to reside in the native VLAN (or default VLAN) of the switch. A data device VLAN (data subnet) is referred to as a port VLAN ID or PVID.