Content

| 8.9 |  | Hands-on Lab Exercises |
| 8.9.9 |  | QoS manually configured FRTS |

| Lab Activity Lab Exercise: QoS Manually Configured Frame Relay Traffic Shaping In this lab, Frame-Relay Traffic Shaping (FRTS) is used to shape traffic exiting a Frame-Relay interface such that it matches the CIR, Bc and Be provided by the ISP.

Lab Activity

e-Lab Activity: QoS Manually Configured Frame Relay Traffic Shaping

This lab activity, Frame-Relay Traffic Shaping (FRTS) is used to shape traffic exiting a Frame-Relay interface such that it matches the CIR, Bc and Be provided by the ISP.