Content

| 3.7 |  | Tuning, Verifying, and Troubleshooting Spanning-Tree Protocol |
| 3.7.7 |  | Verifying STP, RSTP, and MTSP configuration |

Commands for displaying spanning tree status are outlined in Figure .

To display the spanning tree status, use one or more of the privileged EXEC commands shown in Figure .

For information about other keywords for the show spanning-tree privileged EXEC command, refer to the command reference for this release.