Content

| 9.6 |  | Securing User Access |
| 9.6.1 |  | Securing user access |

Management traffic is not the only traffic that needs to be secured in corporate networks. Different types of user traffic, such as user traffic from different parts of the organization, should be separated from each other. User traffic should also be kept separate from management traffic.

User traffic can be controlled using:

- Virtual LANs
- Port security
- Protected ports and private VLANs
- Access Control Lists (ACLs)