Content

| 3.6 |  | STP Configuration |
| 3.6.6 |  | Configuring switch priority of a VLAN |

The switch priority can be configured to make it more likely that the switch will be chosen as the root switch. For most situations, using the spanning-tree vlan vlan-id root primary and the spanning-tree vlan vlan-id root secondary global configuration commands to modify the switch priority is recommended.

Beginning in privileged EXEC mode, follow the steps outlined in Figure to configure the switch priority of a VLAN

To return the switch to its default setting, use the no spanning-tree vlan vlan-id priority global configuration command.