Content

| 2.4 |  | Configuring VLANs and VMPS |
| 2.4.2 |  | Verifying VLAN configuration |

Once a switch has been configured for VLANs, the configuration should be verified with the show vlan brief command. The output example shows that VLAN 2 is configured on module 0, port 3.

When configuring VLANs, keep in mind that:

- A created VLAN remains unused until it is mapped to switch ports.
- The default configuration has all of the switch ports on VLAN 1.