Content

| 6.4 |  | HSRP Configuration |
| 6.4.7 |  | Verify HSRP configuration |

To display the status of the HSRP router, enter the following command in privileged EXEC mode:

> Router#show standby type-number group brief

- Type-number – (Optional) Indicates the target interface type and number for which output is displayed.
- Group – (Optional) Indicates a specific HSRP group on the interface for which output is displayed.
- Brief – (Optional) Displays a single line of output summarizing each standby group.

If none of the optional interface parameters are used, the show standby command will display HSRP information for all interfaces.