Content

| 8.9 |  | Hands-on Lab Exercises |
| 8.9.10 |  | QoS dynamically configured FRTS |

| Lab Activity Lab Exercise: QoS Dynamic Frame Relay Traffic Shaping In this lab, Dynamic Frame-Relay Traffic Shaping (FRTS) is used to shape traffic exiting a Frame-Relay interface such that the traffic flow responds to Backward Explicit Congestion Notification (BECN) received from the Frame-Relay switch.

Lab Activity

e-Lab Activity: QoS Dynamic Frame Relay Traffic Shaping

This lab activity, Dynamic Frame-Relay Traffic Shaping (FRTS) is used to shape traffic exiting a Frame-Relay interface such that the traffic flow responds to Backward Explicit Congestion Notification (BECN) received from the Frame-Relay switch.