RTF#show ip bgp neighbor
BGP neighbor is 172.16.2.254, remote AS 3, internal link
BGP version 4, remote router ID 172.16.2.254
BGP state = Established, table version = 2, up for 22:36:09
Last read 00:00:10, hold time is 180, keepalive interval is 60 seconds 
Minimum time between advertisement runs is 5 seconds
Received 1362 messages, 0 notifications, 0 in queue
Sent 1362 messages, 0 notifications, 0 in queue
Connections established 2; dropped 1
Connection state is ESTAB, I/O status: 1, unread input bytes: 0
Local host: 172.16.1.2, Local port: 11008
Foreign host: 172.16.2.254, Foreign port: 179
BGP neighbor is 192.68.12.1, remote AS 2, external link
BGP version 4, remote router ID 192.68.5.2
BGP state = Established, table version = 2, up for 22:13:01
Last read 00:00:00, hold time is 180, keepalive interval is 60 seconds 
Minimum time between advertisement runs is 30 seconds
Received 1336 messages, 0 notifications, 0 in queue
Sent 1336 messages, 0 notifications, 0 in queue
Connections established 1; dropped 0
External BGP neighbor may be up to 2 hops away.
Connection state is ESTAB, I/O status: 1, unread input bytes: 0
Local host: 192.68.5.1, Local port: 11016
Foreign host: 192.68.12.1, Foreign port: 179
RTF#
