Commands

Modules: | 1 | 2 | 3 | 4 | 5 | 6 | 7 | 8 | 9 | CS 1 | CS 2 | CS 3 | All |

Module 5: EIGRP

5.5.1

Configuring EIGRP for IP Networks

> Router(config)#router eigrp autonomous-system-number
> Router(config-router)#network network-number
> Router(config-if)#bandwidth kilobits
> Router(config-router)#eigrp log-neighbor-changes

5.5.3

The Bandwidth-Percent Command

> Router(config-if)#ip bandwidth-percent eigrp as-number percent

5.5.4

Summarizing EIGRP Routes for IP

> Router(config-router)#no auto-summary

5.5.5

Summarizing EIGRP Routes for IP

> Router(config-if)#ip summary-address eigrp as-number network-address subnet-mask [admin-distance]

5.6.1

Verifying EIGRP Operation

> EIGRP Show Commands:
> Router#show ip eigrp neighbors [type number][details]
> Router#show ip eigrp interfaces [interface-type interface-number][as-number]
> Router#show ip eigrp topology [as-number | [[ip-address] mask]] [active | all-links | pending | summary | zero-successors]
> Router#show ip eigrp traffic [as-number]
> EIGRP Debug Commands:
> Router#debug eigrp fsm
> Router#debug eigrp packet

| Close Window |

| All contents copyright © 2003 Cisco Systems, Inc. All rights reserved.