Output=Router+D%23show+running%2Dconfig%0A%21Router+D%0Arouter+bgp+256%0Aneighbor+3%2E3%2E3%2E4+remote%2Das+300%0Aroute%2Dmap+SETLOCALIN+in%0Aneighbor+128%2E213%2E11%2E1+remote%2Das+256%0A%21%0Aip+as%2Dpath+7+permit+%5E300%24%0Aroute%2Dmap+SETLOCALIN+permit+10%0Amatch+as%2Dpath+7%0Aset+local%2Dpreference+200%0A%21%0Aroute%2Dmap+SETLOCALIN+permit+20%0ARouter+D%23%0A