RTG#show running-config
hostname RTG

ip subnet-zero

interface Loopback0
 ip address 195.211.10.174 255.255.255.192

interface Serial0
 ip address 192.208.10.1 255.255.255.252

interface Serial1
 ip address 195.211.10.1 255.255.255.252

router bgp 500
 network 195.211.10.0
 aggregate-address 195.211.0.0 255.255.0.0 summary-only
 neighbor 192.208.10.2 remote-as 300
 neighbor 192.208.10.2 send-community
 neighbor 192.208.10.2 route-map setcommunity out
 neighbor 195.211.10.2 remote-as 400
!
ip classless
access-list 1 permit 195.211.0.0 0.0.255.255
access-list 2 permit any
access-list 101 permit ip 195.211.0.0 0.0.255.255 host 255.255.0.0
route-map setcommunity permit 20
 match ip address 2
!
route-map setcommunity permit 10
 match ip address 1
 set community no-export

RTG#
