Content

| 4.3 |  | Verifying RIP v2 Operation |
| 4.3.2 |  | Debug commands |

Two configuration problems common to RIP v2 are mismatched versions and misconfigured authentication. Both difficulties are easy to discover with the following debugging commands.

Use the

debug ip rip EXEC command to display information on RIP routing transactions. The no form of this command disables debugging output.

> Router#debug ip rip [events]

Use the

debug ip routing EXEC command to display information on RIP routing table updates and route-cache updates. The no form of this command disables debugging output.

> Router#debug ip routing

| Lab Activity e-Lab Activity: Debug Commands This lab is to learn various useful debug commands and interpret the information given by these commands.