Content

| 8.6 |  | Congestion Avoidance |
| 8.6.4 |  | Verifying WRED configuration |

The following commands can be used to verify the configuration and operation of WRED:

> Router#show interfaces [type slot|port-adapter|port]– Displays WRED configuration on an interface.

> Router#show queueing random-detect – Displays the queuing configuration for WRED.

> Router#show queue interface-type interface-number –Displays the header information of the packets inside a queue.